# Boundaries Constants (Scripting)

Property Name | Property Id | Display Name | Property Kind
AccumulatorNetFlow | 394 | Net Flow | Result
BoundaryFlow | 68 | Flow | Input
BoundaryFlowDirection | 22 | Flow Direction | Input
BoundaryFlowUnit | 34 | Flow Unit | Input
BoundaryPressure | 66 | Pressure | Input
BoundaryPressure | 66 | Surface Pressure | Input
BoundaryPressureUnit | 30 | Pressure Unit | Input
BoundaryTemperature | 64 | Temperature | Input
BoundaryTemperatureUnit | 29 | Temperature Unit | Input
CalculatedDensity | 139 | Density | Result
CalculatedDensity | 139 | In Density | Result
CalculatedHeatTransferred | 180 | Heat Transferred | Result
CalculatedOutDensity | 140 | Out Density | Result
CalculatedOutViscosity | 142 | Out Viscosity | Result
CalculatedQuality | 386 | Calculated Quality (0..1) | Result
CalculatedSpecificHeat | 49 | In Specific Heat Capacity | Result
CalculatedSpecificHeat | 49 | Specific Heat Capacity | Result
CalculatedViscosity | 141 | In Viscosity | Result
CalculatedViscosity | 141 | Viscosity | Result
ComponentDBName | 106 | Sprinkler Name | Input
ComponentDesignPressure | 157 | Exit Pressure | Input
ComponentDesignPressureUnit | 159 | Pressure Unit | Input
ComponentKindStr | 356 | Element Type | Result
ComponentNumber | 0 | -- ID -- | Result
ElementTextAlignment | 303 | Alignment | Input
ElementTextFont | 304 | Font | Input
ElementTextProperties | 305 | Properties | Input
Elevation | 62 | Elevation to Vessel Base | Input
Elevation | 62 | Elevation | Input
ElevationUnit | 28 | Elevation Unit | Input
EnteredKorKfValue | 27 | K (Pressure Loss Coeff) | Input
EquivalentLength | 398 | Equivalent Length (Le/D) | Result
Fluid | 85 | Fluid | Input
FluidMixtureType | 322 | Mix Type | Input
FluidType | 355 | Fluid Type | Input
HeatDirection | 178 | Heat Transfer Direction | Input
HeatLossModel | 105 | Heat Loss Model | Input
HeatTransferred | 179 | Heat Transferred | Input
HeatTransferredUnit | 181 | Heat Transfer Unit | Input
InFlow | 477 | In Flow | Result
InternalFlow | 46 | Flow | Result
InVaporPressure | 195 | In Vapor Pressure | Result
IsStaticPressure | 403 | Pressure Model | Input
JTCoefficient | 453 | Joule-Thomson Coefficient | Result
LiquidLevel | 70 | Liquid Level above Base | Input
LiquidLevelUnit | 31 | Level Unit | Input
MachNumber | 134 | In Mach Number | Result
NNIncludeSizeDistribution | 368 | Use Size Distribution Data | Input
NNSizeD50 | 369 | d50 mean diameter | Input
NNSizeD85 | 380 | d85 (85% of mass finer) | Input
NNSizeM100 | 373 | %Retained 100Mesh (.149mm) | Input
NNSizeM20 | 370 | %Retained 20Mesh (.833mm) | Input
NNSizeM200 | 374 | %Retained 200Mesh (.074mm) | Input
NNSizeM325 | 375 | %Retained 325Mesh (.043mm) | Input
NNSizeM35 | 371 | %Retained 35Mesh (.417mm) | Input
NNSizeM60 | 372 | %Retained 60Mesh (.25mm) | Input
NNSizeM625 | 376 | %Retained 625Mesh (.02mm) | Input
NNSizeUnit | 377 | d50/d85 Size Unit | Input
NNSolid | 357 | Solids | Input
NNSolidBy | 358 | Concentration defined by | Input
NNSolidPercent | 359 | Solids Concentration % | Input
NTPGasFlow | 338 | Flow at NTP | Result
OutCalculatedSpecificHeat | 54 | Out Specific Heat Capacity | Result
OutCrossSectionalArea | 438 | Out Cross Section Flow Area | Result
OutFlow | 478 | Out Flow | Result
OutMachNumber | 135 | Out Mach Number | Result
OutPhaseState | 169 | Out Fluid Phase | Result
OutPiezometricPressure | 53 | Out Piezometric Pressure | Result
OutStagnationPressure | 45 | Out Stagnation Pressure | Result
OutStaticPressure | 55 | Out Static Pressure | Result
OutStaticTemperature | 65 | Out Static Temperature | Result
OutTemperature | 56 | Out Stag. Temperature | Result
OutTwoPhaseQuality | 215 | Out Vapor Quality | Result
OutVaporPressure | 378 | Out Vapor Pressure | Result
OutVelocity | 59 | Out Velocity | Result
OutVelocityPressure | 57 | Out Velocity Pressure | Result
PhaseState | 21 | In Fluid Phase | Result
PiezometricPressure | 48 | In Piezometric Pressure | Result
PiezometricPressure | 48 | Piezometric Pressure | Result
PipeCrossSectionalArea | 381 | In Cross Section Flow Area | Result
PPSolidPercent | 407 | Wt% oven dry concentration | Input
PressureLoss | 58 | Friction Loss | Result
ResultFluid | 199 | Composition % | Result
ResultKValue | 421 | K Value | Result
ResultSolidsDelivered | 429 | Solids Delivered | Result
ShowElementText | 302 | Properties on Flowsheet | Input
SlurryFlowBasis | 321 | Flow Defined By | Input
StagnationPressure | 44 | In Stagnation Pressure | Result
StagnationPressure | 44 | Stagnation Pressure | Result
StagnationPressureLoss | 405 | Stagnation Pressure Loss | Result
StaticPressure | 50 | In Static Pressure | Result
StaticPressure | 50 | Static Pressure | Result
StaticPressureLoss | 387 | Static Pressure Loss | Result
StaticTemperature | 63 | In Static Temperature | Result
Status | 2 | Status | Input
STPGasFlow | 339 | Flow at STP | Result
Temperature | 51 | In Stag. Temperature | Result
Temperature | 51 | Temperature | Result
TemperatureChange | 132 | Temperature Change | Input
TemperatureChangeUnit | 133 | Temperature Unit | Input
TwoPhaseFlowInputQuality | 69 | Quality (0..1) | Input
TwoPhaseQuality | 284 | In Vapor Quality | Result
UniqueName | 84 | Unique Name | Input
UserDefinedFields | 496 | User-Defined Fields | Input
Velocity | 47 | In Velocity | Result
VelocityPressure | 52 | In Velocity Pressure | Result
VesselConnections | 92 | Connections | Input
VesselDiameter | 72 | Vessel Diameter | Input
VesselHeight | 74 | Vessel Full Height | Input
VesselHeightDiameterUnit | 33 | Vessel Dimension Unit | Input
VesselLength | 125 | Vessel Length | Input
VesselType | 91 | Vessel Type | Input
VesselWidth | 123 | Vessel Width | Input