# Pipes Constants (Scripting)

Property Name | Property Id | Display Name | Property Kind
AutoSize | 17 | Sizing Model | Input
CalculatedDensity | 139 | In Density | Result
CalculatedHeatTransferred | 180 | Heat Transferred | Result
CalculatedOutDensity | 140 | Out Density | Result
CalculatedOutViscosity | 142 | Out Viscosity | Result
CalculatedSize | 153 | Exact Economic Size | Result
CalculatedSpecificHeat | 49 | In Specific Heat Capacity | Result
CalculatedViscosity | 141 | In Viscosity | Result
ComponentKindStr | 356 | Element Type | Result
ComponentNumber | 0 | -- ID -- | Result
EconomicVelocity | 42 | Economic Velocity | Result
ElementTextAlignment | 303 | Alignment | Input
ElementTextFont | 304 | Font | Input
ElementTextProperties | 305 | Properties | Input
FinesVolumePercent | 449 | Fines, Xf | Result
FlowScaleFactorPercent | 335 | Scaling (0 to 50%) | Input
FluidShearRate | 406 | Fluid Shear Rate (in s-1) | Result
FrictionFactor | 60 | Friction Factor | Result
FullyStratifiedVolumePercent | 452 | Fully Stratified, Xs | Result
HeatDirection | 178 | Heat Transfer Direction | Input
HeatLossModel | 105 | Heat Loss Model | Input
HeatTransferred | 179 | Heat Transferred | Input
HeatTransferredUnit | 181 | Heat Transfer Unit | Input
HeatTransferUSource | 430 | Heat Transfer Coeff (U Value) | Input
HeterogeneousVolumePercent | 451 | Heterogeneous, Xh | Result
InFlow | 477 | In Flow | Result
InternalFlow | 46 | Flow | Result
InVaporPressure | 195 | In Vapor Pressure | Result
JTCoefficient | 453 | Joule-Thomson Coefficient | Result
MachNumber | 134 | In Mach Number | Result
NTPGasFlow | 338 | Flow at NTP | Result
OutCalculatedSpecificHeat | 54 | Out Specific Heat Capacity | Result
OutCrossSectionalArea | 438 | Out Cross Section Flow Area | Result
OutFlow | 478 | Out Flow | Result
OutMachNumber | 135 | Out Mach Number | Result
OutPhaseState | 169 | Out Fluid Phase | Result
OutPiezometricPressure | 53 | Out Piezometric Pressure | Result
OutsideWallTemperature | 414 | Outside Surface Temperature | Result
OutStagnationPressure | 45 | Out Stagnation Pressure | Result
OutStaticPressure | 55 | Out Static Pressure | Result
OutStaticTemperature | 65 | Out Static Temperature | Result
OutTemperature | 56 | Out Stag. Temperature | Result
OutTwoPhaseQuality | 215 | Out Vapor Quality | Result
OutVaporPressure | 378 | Out Vapor Pressure | Result
OutVelocity | 59 | Out Velocity | Result
OutVelocityPressure | 57 | Out Velocity Pressure | Result
OutVsg | 243 | Out Gas Superficial Velocity | Result
OutVsl | 240 | Out Liq Superficial Velocity | Result
OverallHeatTransferCoeff | 419 | Overall Ht Transfer Coeff | Input
OverallHeatTransferCoefficient | 413 | Overall Ht Transfer Coeff | Result
OverallHeatTransferCoeffUnit | 420 | Heat Transfer Coeff Unit | Input
PhaseState | 21 | In Fluid Phase | Result
PiezometricPressure | 48 | In Piezometric Pressure | Result
PipeAnnulusID | 99 | Annulus Inner Diameter | Input
PipeAnnulusOD | 100 | Annulus Outer Diameter | Input
PipeAnnulusUnit | 101 | Diameter Unit | Input
PipeBackfillThickness | 466 | Buried Backfill Thickness | Input
PipeBackfillType | 465 | Buried Backfill Type | Input
PipeBuriedDepth | 467 | Buried Depth to Pipe Center | Input
PipeClass | 95 | Classification | Input
PipeCoatingThickness | 460 | Pipe Coating Thickness | Input
PipeCoatingType | 459 | Pipe Coating Type | Input
PipeCrossSectionalArea | 381 | In Cross Section Flow Area | Result
PipeDatabaseRoughnessName | 103 | Roughness Description | Input
PipeDatabaseScalingName | 336 | Scaling Description | Input
PipeDepositionVelocity | 439 | Cvd Deposition Velocity | Result
PipeDescription | 107 | Nominal Size | Input
PipeDesignPressureGradient | 426 | Design Pressure Gradient | Input
PipeDesignPressureGradientUnit | 39 | Pressure Gradient Unit | Input
PipeDesignVelocity | 425 | Design Velocity | Input
PipeDesignVelocityUnit | 417 | Velocity Unit | Input
PipeDiameter | 75 | Inside Diameter | Input
PipeDiameterUnit | 35 | Diameter Unit | Input
PipeExactPressureGradientSize | 446 | Exact Pressure Gradient Size | Result
PipeExactVelocitySize | 444 | Exact Velocity Size | Result
PipeFixedFrictionFactor | 116 | Fixed Friction Factor | Input
PipeFrictionModel | 104 | Friction Model | Input
PipeGeometry | 83 | Geometry | Input
PipeHazenWilliamsCoefficient | 81 | Hazen Williams Coeff | Input
PipeInsulation | 108 | Insulation Type | Input
PipeInsulationThickness | 110 | Insulation Thickness | Input
PipeInsulationThickness1 | 463 | Buried Insulation Thickness | Input
PipeInsulationThicknessUnit | 112 | Insulation Thickness Unit | Input
PipeInsulationType | 462 | Buried Insulation Type | Input
PipeLength | 79 | Length | Input
PipeLengthUnit | 37 | Length Unit | Input
PipeLocalAmbientTemperature | 113 | Local Outside Temperature | Input
PipeLocalAmbientTemperatureUnit | 115 | Ambient Temperature Unit | Input
PipeMaxDepositionVelocity | 71 | Deposition Velocity | Result
PipeMaxOpPressure | 306 | Max Op Pressure | Input
PipeMaxOpPressureUnit | 93 | Pressure Unit | Input
PipeOutsideDiameter | 194 | Outside Diameter | Input
PipeRectangularHeight | 97 | Rectangular Height | Input
PipeRectangularUnit | 98 | Width/Height Unit | Input
PipeRectangularWidth | 96 | Rectangular Width | Input
PipeRoughness | 77 | Roughness | Input
PipeRoughnessUnit | 36 | Roughness Unit | Input
PipeSiDiameter | 76 | Size | Result
PipeSizingPressureGradient | 445 | Sizing Pressure Gradient | Result
PipeSizingVelocity | 443 | Sizing Velocity | Result
PipeSoilTemperature | 470 | Average Soil Temperature | Input
PipeSoilTemperatureUnit | 471 | Temperature Unit | Input
PipeSoilType | 469 | Soil Type | Input
PipeSpecificEnergy | 80 | Specific Energy | Result
PipeSurfaceEmissivity | 184 | Surface Emissivity | Input
PipeThickness | 78 | Wall Thickness | Input
PipeThicknessUnit | 468 | Thickness/Depth Units | Input
PipeVisualColor | 24 | Draw Color | Input
PipeVisualThickness | 23 | Draw Thickness [1..5] | Input
PipeWallShearStress | 408 | Wall Shear Stress | Result
PipeWindSpeed | 185 | Local Wind Speed | Input
PipeWindSpeedUnit | 187 | Speed Unit | Input
PressureLoss | 58 | Friction Loss | Result
PressureLossCorrelationName | 340 | Loss Correlation | Result
PseudoHomogeneousVolumePercent | 450 | Pseudo-Homogeneous, Xp | Result
ResultAutoSize | 89 | Result Auto Size | Result
ResultFluid | 199 | Composition % | Result
ResultHeatModel | 415 | Calculated T Type | Result
ResultPressureGradient | 447 | Pressure Gradient | Result
ReynoldsNumber | 61 | Reynolds No | Result
Rinside | 409 | Inside Film Coefficient | Result
Rinsulation | 411 | Insulation Coefficient | Result
Routside | 412 | Outside Film Coefficient | Result
Rwall | 410 | Pipe Wall Coefficient | Result
ShowElementText | 302 | Properties on Flowsheet | Input
SlurryVelocityRatio | 498 | Slurry Velocity Ratio | Result
StagnationPressure | 44 | In Stagnation Pressure | Result
StagnationPressureLoss | 405 | Stagnation Pressure Loss | Result
StaticPressure | 50 | In Static Pressure | Result
StaticPressureLoss | 387 | Static Pressure Loss | Result
StaticTemperature | 63 | In Static Temperature | Result
Status | 2 | Status | Input
STPGasFlow | 339 | Flow at STP | Result
Temperature | 51 | In Stag. Temperature | Result
TemperatureChange | 132 | Temperature Change | Input
TemperatureChangeUnit | 133 | Temperature Unit | Input
TwoPhaseQuality | 284 | In Vapor Quality | Result
UniqueName | 84 | Unique Name | Input
UsePipeBackfill | 464 | Use Buried Backfill | Input
UsePipeCoating | 458 | Use Pipe Coating | Input
UsePipeDatabaseProperties | 82 | Use Database Size | Input
UsePipeDatabaseRoughness | 102 | Use Database Roughness | Input
UsePipeDatabaseScaling | 334 | Use Database Scaling | Input
UsePipeInsulation | 461 | Use Buried Insulation | Input
UsePipeInsulationDatabase | 109 | Use Insulation | Input
UserDefinedFields | 496 | User-Defined Fields | Input
VaporToLiquidMass | 475 | Mass of Vapor Condensed | Result
Velocity | 47 | In Velocity | Result
VelocityPressure | 52 | In Velocity Pressure | Result
Vsg | 237 | In Gas Superficial Velocity | Result
Vsl | 236 | In Liq Superficial Velocity | Result