# Calculation Methods - Known Pressure

There are no specific calculations at known pressure boundaries. FluidFlow always calculates the flow that will be achieved at the known pressure and the flow direction. If the flow is into the network then temperature and mass composition values that you specified via the Input Editor will exist at this point. If the calculated flow direction is out of the network, then the fluid temperature and mass composition is calculated from application of the conservation laws.