# Junctions Constants (Scripting)

Property Name | Property Id | Display Name | Property Kind
BranchJunctionK | 144 | Branch K (based on channel flow) | Result
CalculatedDensity | 139 | Density | Result
CalculatedDensity | 139 | In Density | Result
CalculatedHeatTransferred | 180 | Heat Transferred | Result
CalculatedOutDensity | 140 | Out Density | Result
CalculatedOutViscosity | 142 | Out Viscosity | Result
CalculatedSpecificHeat | 49 | In Specific Heat Capacity | Result
CalculatedSpecificHeat | 49 | Specific Heat Capacity | Result
CalculatedTType | 308 | Calculated T Type | Result
CalculatedViscosity | 141 | In Viscosity | Result
CalculatedViscosity | 141 | Viscosity | Result
ComponentKindStr | 356 | Element Type | Result
ComponentNameIndex | 161 | Bend Defined By | Input
ComponentNameIndex | 161 | Cross Defined By | Input
ComponentNameIndex | 161 | Mitre Defined By | Input
ComponentNameIndex | 161 | Tee Defined By | Input
ComponentNameIndex | 161 | Wye Defined By | Input
ComponentNumber | 0 | -- ID -- | Result
ComponentQuantity | 119 | Quantity | Input
CrossNomenclature | 314 | Nomenclature | Input
CrossStraightPipeExitNumber | 315 | Straight Pipe (YELLOW) | Input
DirectionalExitPipeNumber | 19 | Branch Pipe (RED) | Input
DirectionalExitPipeNumber | 19 | Channel Pipe (RED) | Input
ElementTextAlignment | 303 | Alignment | Input
ElementTextFont | 304 | Font | Input
ElementTextProperties | 305 | Properties | Input
Elevation | 62 | Elevation | Input
ElevationUnit | 28 | Elevation Unit | Input
EquivalentLength | 398 | Equivalent Length (Le/D) | Result
HeatDirection | 178 | Heat Transfer Direction | Input
HeatLossModel | 105 | Heat Loss Model | Input
HeatTransferred | 179 | Heat Transferred | Input
HeatTransferredUnit | 181 | Heat Transfer Unit | Input
InFlow | 477 | In Flow | Result
InternalFlow | 46 | Channel Flow | Result
InternalFlow | 46 | Flow | Result
InVaporPressure | 195 | In Vapor Pressure | Result
JTCoefficient | 453 | Joule-Thomson Coefficient | Result
JunctionBranchAngle | 117 | Branch Angle | Input
JunctionBranchAngle | 117 | Branch/Branch Angle | Input
JunctionBranchAngle | 117 | Mitre Angle | Input
JunctionBranchAngle | 117 | Straight/Branch Angle | Input
JunctionBranchFlow | 317 | Branch Flow | Result
JunctionBranchLoss | 176 | Branch Loss | Result
JunctionBranchReference | 311 | Branch Reference | Result
JunctionConstruction | 122 | Construction | Input
JunctionNomenclature | 313 | Nomenclature | Input
JunctionRD | 118 | R/D Ratio | Input
JunctionSide1Flow | 273 | Side 1 Flow | Result
JunctionSide1Loss | 40 | Side 1 Loss | Result
JunctionSide1Reference | 310 | Side 1 Reference | Result
JunctionSide2Flow | 248 | Side 2 Flow | Result
JunctionSide2Loss | 20 | Side 2 Loss | Result
JunctionSide2Reference | 309 | Side 2 Reference | Result
JunctionStraightFlow | 318 | Straight Flow | Result
JunctionStraightLoss | 216 | Straight Loss | Result
JunctionStraightReference | 312 | Straight Reference | Result
MachNumber | 134 | In Mach Number | Result
NTPGasFlow | 338 | Channel Flow at NTP | Result
NTPGasFlow | 338 | Flow at NTP | Result
NTPJunctionBranchFlow | 361 | Branch Flow at NTP | Result
NTPJunctionSide1Flow | 365 | Side 1 Flow at NTP | Result
NTPJunctionSide2Flow | 367 | Side 2 Flow at NTP | Result
NTPJunctionStraightFlow | 363 | Straight Flow at NTP | Result
OutCalculatedSpecificHeat | 54 | Out Specific Heat Capacity | Result
OutCrossSectionalArea | 438 | Out Cross Section Flow Area | Result
OutFlow | 478 | Out Flow | Result
OutMachNumber | 135 | Out Mach Number | Result
OutPhaseState | 169 | Out Fluid Phase | Result
OutPiezometricPressure | 53 | Out Piezometric Pressure | Result
OutStagnationPressure | 45 | Out Stagnation Pressure | Result
OutStaticPressure | 55 | Out Static Pressure | Result
OutStaticTemperature | 65 | Out Static Temperature | Result
OutTemperature | 56 | Out Stag. Temperature | Result
OutTwoPhaseQuality | 215 | Out Vapor Quality | Result
OutVaporPressure | 378 | Out Vapor Pressure | Result
OutVelocity | 59 | Out Velocity | Result
OutVelocityPressure | 57 | Out Velocity Pressure | Result
PhaseState | 21 | In Fluid Phase | Result
PiezometricPressure | 48 | In Piezometric Pressure | Result
PipeCrossSectionalArea | 381 | In Cross Section Flow Area | Result
PressureLoss | 58 | Friction Loss | Result
ResultFluid | 199 | Composition % | Result
ResultKValue | 421 | K Value | Result
ShowElementText | 302 | Properties on Flowsheet | Input
Side1JunctionK | 124 | Side 1 K (based on channel flow) | Result
Side2JunctionK | 126 | Side 2 K (based on channel flow) | Result
StagnationPressure | 44 | Channel Stagnation Pressure | Result
StagnationPressure | 44 | In Stagnation Pressure | Result
StagnationPressure | 44 | Stagnation Pressure | Result
StagnationPressureLoss | 405 | Stagnation Pressure Loss | Result
StaticPressure | 50 | In Static Pressure | Result
StaticPressureLoss | 387 | Static Pressure Loss | Result
StaticTemperature | 63 | In Static Temperature | Result
Status | 2 | Status | Input
STPGasFlow | 339 | Channel Flow at STP | Result
STPGasFlow | 339 | Flow at STP | Result
STPJunctionBranchFlow | 360 | Branch Flow at STP | Result
STPJunctionSide1Flow | 364 | Side 1 Flow at STP | Result
STPJunctionSide2Flow | 366 | Side 2 Flow at STP | Result
STPJunctionStraightFlow | 362 | Straight Flow at STP | Result
StraightJunctionK | 151 | Straight K (based on channel flow) | Result
Temperature | 51 | In Stag. Temperature | Result
Temperature | 51 | Temperature | Result
TemperatureChange | 132 | Temperature Change | Input
TemperatureChangeUnit | 133 | Temperature Unit | Input
TwoPhaseQuality | 284 | In Vapor Quality | Result
UniqueName | 84 | Unique Name | Input
UserDefinedFields | 496 | User-Defined Fields | Input
Velocity | 47 | In Velocity | Result
VelocityPressure | 52 | In Velocity Pressure | Result