# Calculation Methods - Reservoir

There are no specific calculations at reservoir boundaries. FluidFlow always calculates the flow that will be achieved at the reservoir and the flow direction for each connection. If the flow is into the network then temperature and mass composition values that you specified via the Input Editor will exist at this point. If the calculated flow direction is into the reservoir, then the fluid temperature and mass composition is calculated from application of the conservation laws.