# Calculation Options Dialog

# Pulp & Paper Stock quids If the Slurry module is active then a new tabbed page is added to the default Calculations Options Dialog (F2 key). Pulp & Paper Stock Pressure Loss Correlation: This drop-down menu allows users to choose from two correlation methods: ▪TAPPI. ▪Moller K. TAPPI Pressure Loss Method: If you have selected "TAPPI" as the preferred pressure loss correlation option, you can then choose from a range of pre-defined pulp types stored in the software database. The description of these pulp types is as follows: ▪Unbeaten aspen, sulfite never dried. ▪Long-fibered kraft, never dried CSF 725. ▪Long-fibered kraft, never dried CSF 650. ▪Long-fibered kraft, never dried CSF 550. ▪Long-fibered kraft, never dried CSF 260. ▪Bleached kraft pine, dried and reslurried. ▪Kraft birch, dried and reslurried. ▪Stone groundwood, CSF 114. ▪Refiner groundwood, CSF 150. ▪Newsprint broke, CSF 75. ▪Refiner groundwood (hardboard). ▪Refiner groundwood (insulating board). ▪Hardwood NSSC, CSF 620. ▪Long-fibered kraft, dried and reslurried. ▪Bleached kraft pine, dried and reslurried (SS Pipe). ▪Long-fibered kraft pine, never dried CSF 725 (SS Pipe). where: CSF: is the Canadian Standard Freeness. Moller Pressure Loss Method: If you have selected "Moller K" as the preferred pressure loss correlation option, you simply enter the values for Fiber Aspect Ratio and Freeness of Pulp.