# Booster Data Record

Booster Data Record Group: Integer; Name: String; Manufacturer: String; Component: Integer; Parent: Integer; Materials: Integer; Applications: Integer; BlobData: AddInfo: Impeller: Double; MinImpeller: Double; MaxImpeller: Double; ImpellerUnit: Integer; Speed: Double; MinSpeed: Double; MaxSpeed: Double; InletSize: Double; OutletSize: Double; SizeUnit: Integer; MaxCurveFlow: Double; MaxCurveHead: Double; MaxOpPressure: Double; OpPressureUnit: Integer; ReservedI1: Integer; UseInternalEfficiencyCorrection: Integer; GasConditionVolumeFlow: Integer; Usages: Integer; cCurveFit: EqnType: Integer; PolyOrder: Integer; XUnit: Integer; YUnit: Integer; XSiUnit: Integer; YSiUnit: Integer; CorrelationCoefficientOrYieldStress: Double; XGroup: Integer; YGroup: Integer; DoFitAsSI: Boolean; UseXCrossConvert: Boolean; UseYCrossConvert: Boolean; MinLimit: Double; MaxLimit: Double; MaxAllowablePolyOrder: Integer; AllowNegativeX: Boolean; eCurveFit: EqnType: Integer; PolyOrder: Integer; XUnit: Integer; YUnit: Integer; XSiUnit: Integer; YSiUnit: Integer; CorrelationCoefficientOrYieldStress: Double; XGroup: Integer; YGroup: Integer; DoFitAsSI: Boolean; UseXCrossConvert: Boolean; UseYCrossConvert: Boolean; MinLimit: Double; MaxLimit: Double; MaxAllowablePolyOrder: Integer; AllowNegativeX: Boolean; nCurveFit: EqnType: Integer; PolyOrder: Integer; XUnit: Integer; YUnit: Integer; XSiUnit: Integer; YSiUnit: Integer; CorrelationCoefficientOrYieldStress: Double; XGroup: Integer; YGroup: Integer; DoFitAsSI: Boolean; UseXCrossConvert: Boolean; UseYCrossConvert: Boolean; MinLimit: Double; MaxLimit: Double; MaxAllowablePolyOrder: Integer; AllowNegativeX: Boolean;