# General Resistances Constants (Scripting)

Property Name | Property Id | Display Name | Property Kind
CalculatedDensity | 139 | In Density | Result
CalculatedHeatTransferred | 180 | Heat Transferred | Result
CalculatedOutDensity | 140 | Out Density | Result
CalculatedOutViscosity | 142 | Out Viscosity | Result
CalculatedSpecificHeat | 49 | In Specific Heat Capacity | Result
CalculatedViscosity | 141 | In Viscosity | Result
CentrifugeCoefficient | 348 | Centrifuge Coefficient | Input
CentrifugeRadiusE | 345 | External Radius | Input
CentrifugeRadiusI | 346 | Internal Radius | Input
CentrifugeRadiusUnit | 347 | Radius Unit | Input
CentrifugeSpeed | 344 | Operating Speed (RPM) | Input
CoilDiameter | 245 | Coil Diameter | Input
CoilLength | 247 | Coil Length | Input
CoilSizeUnit | 249 | Coil Size Unit | Input
ComponentDBName | 106 | Filter Name | Input
ComponentDBName | 106 | K Component Name | Input
ComponentDBName | 106 | Kf Component Name | Input
ComponentDBName | 106 | Kv Component Name | Input
ComponentKindStr | 356 | Element Type | Result
ComponentNumber | 0 | -- ID -- | Result
ComponentQuantity | 119 | Quantity | Input
ConstantHeadLoss | 154 | Pressure Loss (Constant) | Input
ConstantHeadLossUnit | 156 | Pressure Loss Unit | Input
CycloneCalculationDefinition | 230 | Cyclone Loss Correlation | Input
CycloneDiameter | 231 | Cyclone Diameter (Dc) | Input
CycloneInletDiameter | 242 | Inlet Dia (typically Dc/2) | Input
CycloneInletGeometry | 241 | Inlet Geometry | Input
CycloneInletWidth | 232 | Inlet W (typically Dc/4) | Input
CycloneK | 234 | Cyclone Miller K | Input
CycloneLappleK | 238 | Cyclone Shepherd K | Input
CycloneOutletDiameter | 239 | Outlet Dia (typically Dc/2) | Input
CycloneSizeUnit | 229 | Size Unit | Input
CyloneInletHeight | 233 | Inlet H (typically Dc/2) | Input
ElementTextAlignment | 303 | Alignment | Input
ElementTextFont | 304 | Font | Input
ElementTextProperties | 305 | Properties | Input
Elevation | 62 | Elevation | Input
ElevationUnit | 28 | Elevation Unit | Input
EnteredKorKfValue | 27 | K (Pressure Loss Coeff) | Input
EnteredKorKfValue | 27 | Kf (L/D) | Input
EquivalentLength | 398 | Equivalent Length (Le/D) | Result
ExchangerBaffleCount | 264 | Number of Baffles | Input
ExchangerBaffleDistance | 265 | Distance between Baffles | Input
ExchangerBaffleShellDistanceUnit | 269 | Distance/Diameter Unit | Input
ExchangerPassCount | 251 | Number of Tube Passes | Input
ExchangerPitchSize | 259 | Tube Pitch Distance | Input
ExchangerPitchTubeSizeUnit | 263 | Tube Size Unit | Input
ExchangerPitchType | 258 | Tube Pitch Type | Input
ExchangerShellID | 267 | Shell Inside Diameter | Input
ExchangerTubeCount | 250 | Number of Tubes | Input
ExchangerTubeDiameter | 252 | Tube Diameter | Input
ExchangerTubeDiameterUnit | 254 | Diameter Unit | Input
ExchangerTubeLength | 255 | Tube Length | Input
ExchangerTubeLengthUnit | 257 | Length Unit | Input
ExchangerTubeOD | 261 | Tube Outside Diameter | Input
ExpansionJointType | 244 | Expansion Type | Input
ExpansionLoopDimensionsUnit | 474 | Width/Height Units | Input
ExpansionLoopHeight | 473 | Expansion Loop Height | Input
ExpansionLoopWidth | 472 | Expansion Loop Width | Input
HeatDirection | 178 | Heat Transfer Direction | Input
HeatLossModel | 105 | Heat Loss Model | Input
HeatTransferred | 179 | Heat Transferred | Input
HeatTransferredUnit | 181 | Heat Transfer Unit | Input
InFlow | 477 | In Flow | Result
InlineFilterHoleAreaRatio | 120 | Hole/Total Area Ratio | Input
InternalFlow | 46 | Flow | Result
InVaporPressure | 195 | In Vapor Pressure | Result
JTCoefficient | 453 | Joule-Thomson Coefficient | Result
KLossBasis | 114 | Loss Basis | Input
KvExponent | 193 | Exponent | Input
KvFlow | 183 | Flow | Input
KvFlowUnit | 188 | Flow Unit | Input
KvPressureLoss | 189 | Pressure Loss | Input
KvPressureLossUnit | 190 | Pressure Loss Unit | Input
KvRefDensity | 191 | Reference Density | Input
KvRefDensityUnit | 192 | Density Unit | Input
LabyrinthAreaUnit | 354 | Area Unit | Input
LabyrinthInOutCoefficient | 351 | In/Out Loss Coefficient | Input
LabyrinthLeakageArea | 352 | Leakage Area | Input
LabyrinthLengthUnit | 353 | Dimension Unit | Input
LabyrinthRadialClearance | 350 | Radial Clearance | Input
LabyrinthTotalLength | 349 | Length of Labyrinth | Input
MachNumber | 134 | In Mach Number | Result
MeanParticleDiameter | 220 | Mean Particle Diameter | Input
NTPGasFlow | 338 | Flow at NTP | Result
OutCalculatedSpecificHeat | 54 | Out Specific Heat Capacity | Result
OutCrossSectionalArea | 438 | Out Cross Section Flow Area | Result
OutFlow | 478 | Out Flow | Result
OutMachNumber | 135 | Out Mach Number | Result
OutPhaseState | 169 | Out Fluid Phase | Result
OutPiezometricPressure | 53 | Out Piezometric Pressure | Result
OutStagnationPressure | 45 | Out Stagnation Pressure | Result
OutStaticPressure | 55 | Out Static Pressure | Result
OutStaticTemperature | 65 | Out Static Temperature | Result
OutTemperature | 56 | Out Stag. Temperature | Result
OutTwoPhaseQuality | 215 | Out Vapor Quality | Result
OutVaporPressure | 378 | Out Vapor Pressure | Result
OutVelocity | 59 | Out Velocity | Result
OutVelocityPressure | 57 | Out Velocity Pressure | Result
PackedBedDiameter | 226 | Bed Diameter | Input
PackedBedDiameterUnit | 228 | Diameter Unit | Input
PackedBedHeight | 222 | Bed Height | Input
PackedBedHeightUnit | 223 | Height Unit | Input
ParticleDiameterUnit | 221 | Particle Diameter Unit | Input
PhaseState | 21 | In Fluid Phase | Result
PiezometricPressure | 48 | In Piezometric Pressure | Result
PipeCrossSectionalArea | 381 | In Cross Section Flow Area | Result
PressureLoss | 58 | Friction Loss | Result
ResultFluid | 199 | Composition % | Result
ResultKValue | 421 | K Value | Result
ShowElementText | 302 | Properties on Flowsheet | Input
StagnationPressure | 44 | In Stagnation Pressure | Result
StagnationPressureLoss | 405 | Stagnation Pressure Loss | Result
StaticPressure | 50 | In Static Pressure | Result
StaticPressureLoss | 387 | Static Pressure Loss | Result
StaticTemperature | 63 | In Static Temperature | Result
Status | 2 | Status | Input
STPGasFlow | 339 | Flow at STP | Result
Temperature | 51 | In Stag. Temperature | Result
TemperatureChange | 132 | Temperature Change | Input
TemperatureChangeUnit | 133 | Temperature Unit | Input
TwoPhaseQuality | 284 | In Vapor Quality | Result
UniqueName | 84 | Unique Name | Input
UseComponentDatabase | 138 | Use K from Database | Input
UseComponentDatabase | 138 | Use Kf from Database | Input
UseComponentDatabase | 138 | Use Kv from Database | Input
UserDefinedFields | 496 | User-Defined Fields | Input
Velocity | 47 | In Velocity | Result
VelocityPressure | 52 | In Velocity Pressure | Result
VoidFraction | 219 | Particle Void Fraction | Input