# Size Change Constants (Scripting)

Property Name | Property Id | Display Name | Property Kind
AutoSize | 17 | Automatically Size | Input
AutoSizeType | 111 | Sizing Model | Input
CalculatedDensity | 139 | In Density | Result
CalculatedHeatTransferred | 180 | Heat Transferred | Result
CalculatedOutDensity | 140 | Out Density | Result
CalculatedOutViscosity | 142 | Out Viscosity | Result
CalculatedSize | 153 | Calculated Size | Result
CalculatedSpecificHeat | 49 | In Specific Heat Capacity | Result
CalculatedViscosity | 141 | In Viscosity | Result
ComponentKindStr | 356 | Element Type | Result
ComponentNumber | 0 | -- ID -- | Result
ElementTextAlignment | 303 | Alignment | Input
ElementTextFont | 304 | Font | Input
ElementTextProperties | 305 | Properties | Input
Elevation | 62 | Elevation | Input
ElevationUnit | 28 | Elevation Unit | Input
EquivalentLength | 398 | Equivalent Length (Le/D) | Result
HeatDirection | 178 | Heat Transfer Direction | Input
HeatLossModel | 105 | Heat Loss Model | Input
HeatTransferred | 179 | Heat Transferred | Input
HeatTransferredUnit | 181 | Heat Transfer Unit | Input
InFlow | 477 | In Flow | Result
InternalFlow | 46 | Flow | Result
InVaporPressure | 195 | In Vapor Pressure | Result
JTCoefficient | 453 | Joule-Thomson Coefficient | Result
MachNumber | 134 | In Mach Number | Result
NTPGasFlow | 338 | Flow at NTP | Result
OrificeCornerLoss | 341 | Corner Tap Loss | Result
OrificeD2Loss | 457 | D and D/2 Tap Loss | Result
OrificeEqn | 146 | Nozzle Equation | Input
OrificeEqn | 146 | Orifice Equation | Input
OrificeFlangeLoss | 456 | Flange Tap Loss | Result
OrificeSize | 143 | Orifice Size | Input
OrificeSize | 143 | Throat Diameter | Input
OrificeSizeUnit | 145 | Diameter Unit | Input
OrificeSizeUnit | 145 | Orifice Unit | Input
OrificeSizeUnit | 145 | Size Unit | Input
OutCalculatedSpecificHeat | 54 | Out Specific Heat Capacity | Result
OutCrossSectionalArea | 438 | Out Cross Section Flow Area | Result
OutFlow | 478 | Out Flow | Result
OutMachNumber | 135 | Out Mach Number | Result
OutPhaseState | 169 | Out Fluid Phase | Result
OutPiezometricPressure | 53 | Out Piezometric Pressure | Result
OutStagnationPressure | 45 | Out Stagnation Pressure | Result
OutStaticPressure | 55 | Out Static Pressure | Result
OutStaticTemperature | 65 | Out Static Temperature | Result
OutTemperature | 56 | Out Stag. Temperature | Result
OutTwoPhaseQuality | 215 | Out Vapor Quality | Result
OutVaporPressure | 378 | Out Vapor Pressure | Result
OutVelocity | 59 | Out Velocity | Result
OutVelocityPressure | 57 | Out Velocity Pressure | Result
PhaseState | 21 | In Fluid Phase | Result
PiezometricPressure | 48 | In Piezometric Pressure | Result
PipeCrossSectionalArea | 381 | In Cross Section Flow Area | Result
PressureLoss | 58 | Friction Loss | Result
ReducerLength | 137 | Reducer Length | Input
ReducerLengthUnit | 136 | Length Unit | Input
ReducerType | 201 | Reducer Type | Input
ResultFluid | 199 | Composition % | Result
ResultKValue | 421 | K Value | Result
SelectionDesignFlow | 147 | Design Flow | Input
SelectionDesignFlowUnit | 149 | Flow Unit | Input
SelectionDesignPressureLoss | 150 | Design Pressure Change | Input
SelectionDesignPressureLossUnit | 152 | Pressure Change Unit | Input
ShowElementText | 302 | Properties on Flowsheet | Input
StagnationPressure | 44 | In Stagnation Pressure | Result
StagnationPressureLoss | 405 | Stagnation Pressure Loss | Result
StaticPressure | 50 | In Static Pressure | Result
StaticPressureLoss | 387 | Static Pressure Loss | Result
StaticTemperature | 63 | In Static Temperature | Result
Status | 2 | Status | Input
STPGasFlow | 339 | Flow at STP | Result
Temperature | 51 | In Stag. Temperature | Result
TemperatureChange | 132 | Temperature Change | Input
TemperatureChangeUnit | 133 | Temperature Unit | Input
ThickOrificeLength | 283 | Plate Thickness | Input
TwoPhaseQuality | 284 | In Vapor Quality | Result
UniqueName | 84 | Unique Name | Input
UseComponentDatabase | 138 | Use Database Length | Input
UserDefinedFields | 496 | User-Defined Fields | Input
Velocity | 47 | In Velocity | Result
VelocityPressure | 52 | In Velocity Pressure | Result
VenturiInletAngle | 441 | Throat Inlet Angle | Input
VenturiOutletAngle | 442 | Throat Outlet Angle | Input
VenturiThroatLength | 440 | Throat Length | Input