# Calculation Methods - Known Flow

There are no specific calculations at known flow boundaries. FluidFlow always calculates the pressure that will be achieved at the known flow and specified flow direction. If the flow is into the network then temperature and mass composition values that you specified via the Input Editor will exist at this point. If the specified flow direction is out of the network, then the fluid temperature and mass composition is calculated from application of the conservation laws.