# Non-Newtonian Calculations

The Slurry module allows you simulate the flow of two types of non-Newtonian liquids: •non-Newtonian / non-settling •settling slurries with a Newtonian carrier fluid Foods, wastewater and pharmaceutical flows are generally non-Newtonian / non-settling. Mining flows may also be non-Newtonian/non-settling but also include settling slurries, i.e., a Newtonian carrier fluid or vehicle (usually water) with a solids component which may be in full or partial suspension. The Slurry module provides a range of pipe flow friction loss models for simulating these types of flow.