# Valve Data Record

Valve Data Record Group: Integer; Name: String; Manufacturer: String; Component: Integer; Parent: Integer; Materials: Integer; Applications: Integer; BlobData: (Note, the data below can be repeated any number of times) %Open: Integer Cv: Double AddInfo: DefinedBy: Integer; Connections: Integer; multiwayType: Integer; FullyOpenKOrKfOrCv: Double; DivertKOrKfOrCv: Double; Size: Double; SizeUnit: Integer; CurveFit: EqnType: Integer; PolyOrder: Integer; XUnit: Integer; YUnit: Integer; XSiUnit: Integer; YSiUnit: Integer; CorrelationCoefficientOrYieldStress: Double; XGroup: Integer; YGroup: Integer; DoFitAsSI: Boolean; UseXCrossConvert: Boolean; UseYCrossConvert: Boolean; MinLimit: Double; MaxLimit: Double; MaxAllowablePolyOrder: Integer; AllowNegativeX: Boolean; OpPressureUnit: Integer ReservedI1: Integer; MaxOpPressure: Double; ReservedD1: Double;