# Rotating a component

To rotate a component (or a number of components) either: ▪Select the component(s) and use the Ctrl Key AND the "R" key together. ▪Select the component(s), right mouse-click and select Rotate Node (See Figure 1). Figure 1: Rotate Node. You can rotate a group of components on the flowsheet if more than one flowsheet element is selected. See the flowsheet section on multi-selections for information on how to make multiple node and pipe selections. When the flowsheet is set up in orthogonal mode, you can rotate components through steps of 90o. If you have the flowsheet set up in isometric mode, components can be rotated through 30o steps.